Larix Broadcaster

Send SRT with Iphone& IPAD over the mobile network (4G)
(also available for Android)

You can use Larix Groove Website, for generating your setting and just email/whatsapp the settings as mail, message or QR code to your mobile device, or enter them manually
Larix Briadcaster Settings
With the RED Button, you are starting to send SRT.

Settings

With the Gearweehl you go eiter to Connections or settings for compression, latency, audio, video etc.

Connections

settings for IP:Port, latency

or choose settings for video, compression, latency, audio etc.
With the RED Button, you are starting to send SRT.

Larix Broadcaster, tested works perfect, free Haivision Play , tested for 1 min, worked, free